From f5d3ee099170e1a3812923172fa1c77049d83abf Mon Sep 17 00:00:00 2001
From: thing1 <thing1@seacrossedlovers.xyz>
Date: Wed, 2 Apr 2025 15:17:19 +0000
Subject: made the design objectives

---
 electronics/cw2/writeup.tex | 70 +++++++++++++++++++++++++++++++++++++++------
 1 file changed, 62 insertions(+), 8 deletions(-)

(limited to 'electronics/cw2/writeup.tex')

diff --git a/electronics/cw2/writeup.tex b/electronics/cw2/writeup.tex
index aeaae5f..6e69089 100644
--- a/electronics/cw2/writeup.tex
+++ b/electronics/cw2/writeup.tex
@@ -71,14 +71,21 @@ The design should focus on simplicity, as less points of failure should result i
 To evaluate my system at the end, I will comapre it against the following goals
 
 \begin{center}
-	\begin{tabular}{ |c|c| } 
+	\begin{tabular}{ |c| } 
 		\hline
-		objective & how \\ 
+		objective \\ 
+		\hline
+		\hline
+                Can recive radio waves \\
+		\hline
+                Displays the intensity of the volume output by the signal \\
+		\hline
+                Can output the sound of the demodulated waves \\
 		\hline
-                Outputs sound based on the input, that is equivalent to the input & The full system\\
-                Displays the intensity of the volume output by the signal & Use a micro controller \\
-                in & out \\
-                in & out \\
+		\hline
+                Can recevie radio waves beween 50hz and 8Khz \\
+		\hline
+                The audio intesity bar will be at set 0v 2v 4v and 5v \\
 		\hline
 	\end{tabular}
 \end{center}
@@ -514,10 +521,57 @@ As the trace shows, it is negative, a DC offset has been applied. I originally b
 \subsection{User Manual}
 % did it work, how well, compare to original goal
 \section{Evaluation} 
+Here is a repeat of my design objectives to compare against:
+\begin{center}
+\begin{tabular}{ |c| } 
+    \hline
+    objective \\ 
+    \hline
+    \hline
+            Can recive radio waves \\
+    \hline
+            Displays the intensity of the volume output by the signal \\
+    \hline
+            Can output the sound of the demodulated waves \\ 
+    \hline
+    \hline
+            Can recevie radio waves beween 50hz and 8Khz \\
+    \hline
+            The audio intesity bar will be at set 0v 2v 4v and 5v \\
+    \hline
+\end{tabular}
+
+Here is how I achieved each of them:
+
+\begin{tabular}{ |c| } 
+    \hline
+    how did I achieve it\\ 
+    \hline
+    \hline
+            I used a simple radio receiver made with a capacitor and an inductor \\
+    \hline
+            Using a micro controller and a bar graph \\
+    \hline
+            Using a push pull power amp and speaker\\
+    \hline
+    \hline
+            By using the correct part values on my recevier to ensure it has the correct break freqency\\
+    \hline
+            By programing my micro controller to have the set values \\
+    \hline
+\end{tabular}
+\end{center}
+
+This shows that I have achieved all of my design goals.
+
 \subsection{What went well?}
 My system worked as intended, it did play the input signal, through the speakers, atfer passing through all the subsystems and the speaker.
-I will compare, line by line, to my design objectives here:
-
+For this I believe I made a good project.
 \subsection{What didn't go well?}
+My colour coding for my system was not ideal, I believe it was too generic and would have benififted from using multiple colours for each sub system. 
+
+I would have prefered to use a less noisy alternative to the push pull power amp, as my system outputed a large amount of static.
+
+I would have prefered to use FM rather than AM, as this would reduce the noise; making the device better.
 } 
 \end{document}
-- 
cgit v1.2.3

